Before using the mft do the following steps to to give the app permissionto use the usb device

	1. Copy the mft.rules file to /etc/udev/rules.d
	2. Reload the udev rules:  udevadm control --reload-rules && udevadm trigger
